FloppyControl firmware commands

|  |  |  |  |
| --- | --- | --- | --- |
| **Cmd** | **Description** | **Cmd** | **Description** |
| q | Deselect drive | a | Select drive |
| w | Disable motor | s | Enable motor |
| e | DIR = 1 = backwards | d | DIR = 0 = forewards |
| r | STEP = 1 | f | STEP = 0 |
| t | Next track (single STEP=0;STEP=1) | g | Previous track |
| h | Side = 1 | j | Side = 0 |
| . | Stop capture | , | Resume capture |
| [ | Increment/cycle through microsteppings | ] | reset microstepping to full step |
| y | Next track based on microstepping | 0 | Seek TRK00 |
| i | Display info, text in ascii |  |  |